This tool can be used to create a hexagonal vector grid. The extent of the hexagonal grid is based on the extent of an input vector base file (`base`). The user must also specify the hexagonal cell width (`width`) and whether the hexagonal orientation (`orientation`) is `horizontal` or `vertical`. To use a raster base image instead of a vector, use the hexagonal_grid_from_raster_base tool.

## See Also

hexagonal_grid_from_raster_base

## Function Signature

`def hexagonal_grid_from_vector_base(self, base: Vector, width: float, orientation: str = "h") -> Vector: ...`

## Project Links

WbW Homepage User Manual Support WbW