[general]
name=XYZ/MGRS Coordinate Tool
qgisMinimumVersion=3.0
qgisMaximumVersion=4.99
description=Advanced multi-format coordinate tool supporting XYZ tiles, MGRS, WKT, WKB, and GeoJSON with interactive navigation and visualization. Part of MAS Raster Processing tools. 
version=1.0.1
author=Mirjan Ali Sha
email=mastools.help@gmail.com

about=Professional multi-format coordinate capture and visualization tool for QGIS. Supports 5 coordinate systems with full navigation and plotting capabilities.
    .
    SUPPORTED FORMATS:
    - XYZ Tiles: Web mapping tile coordinates with zoom levels (Red visualization)
    - MGRS: Military Grid Reference System, Sentinel-2 compatible (Blue visualization)
    - WKT: Well-Known Text geometry format (Green visualization)
    - WKB: Well-Known Binary geometry as hex string (Yellow visualization)
    - GeoJSON: JSON-based geometry format (Purple visualization)
    .
    KEY FEATURES:
    - Interactive map clicking with crosshair cursor for coordinate capture
    - Dual-mode operation: Click-to-capture OR manual input for all formats
    - Go To button: Navigate/zoom to any coordinate system location
    - Plot Polygon/Geometry button: Visualize geometries with color-coded layers
    - Editable coordinate inputs (X, Y, Z for tiles; text input for others)
    - Smart geometry type detection (Point, LineString, Polygon, Multi types)
    - Dockable widget interface with system dropdown selector
    - Seamless integration with MAS Raster Processing toolbar
    - Coordinate reprojection support for different CRS
    - Memory layer creation with proper attribute tables and symbology
    .
    QUICK START GUIDE:
    1. Activate tool: Click XYZ Coordinate Tool icon or Raster menu - MAS Raster Processing - XYZ Coordinate Tool
    2. Select coordinate system from dropdown (XYZ Tiles, MGRS, WKT, WKB, or GeoJSON/JSON)
    3. FOR XYZ/MGRS: Click on map to capture coordinates. FOR WKT/WKB/GEOJSON: Paste or type geometry string in the input field
    4. Click Go To to navigate to the location
    5. Click Plot Polygon to visualize the geometry on map
    6. Edit coordinates manually if needed (all inputs are editable)
    .
    USE CASES:
    - Tile-based web mapping applications (XYZ tiles)
    - Sentinel-2 satellite imagery tile identification (MGRS)
    - Geometry data exchange and validation (WKT, WKB, GeoJSON)
    - Coordinate reference system testing and debugging
    - Geospatial data quality assurance workflows
    - Educational tool for understanding different coordinate formats
    .
    TECHNICAL NOTES:
    - XYZ tiles: Z value (zoom level) range 0-22, default 14
    - MGRS: Fixed latitude band calculation with 2,000,000m cycle handling
    - WKT/WKB/GeoJSON: Automatic geometry type detection and appropriate symbology
    - All geometries are created in EPSG:4326 (WGS84) coordinate system
    - Color-coded layers for easy identification of coordinate system source
    .
    Please rate this plugin based on your experience - your feedback motivates continued development!
    For support, feature requests, or custom QGIS tools: mastools.help@gmail.com
    MAS = Mirjan Ali Sha (plugin author)

tracker=https://github.com/Mirjan-Ali-Sha/xyz-coordinate-tool/issues
repository=https://github.com/Mirjan-Ali-Sha/xyz-coordinate-tool
tags=coordinates,xyz,tiles,mgrs,wkt,wkb,geojson,navigation,raster,geospatial,mapping,sentinel,geometry,conversion,visualization
homepage=https://github.com/Mirjan-Ali-Sha/xyz-coordinate-tool
category=Raster
icon=icon.png
experimental=False
deprecated=False

hasProcessingProvider=no
hasWebMapServices=no

changelog=Version 1.0.0 (2025-11-29)

    1.0.1 - 2026-08-09
        • QGIS 4 and Qt6 compatibility updates
        • Fixed all Bandit security audit issues
    - MAJOR UPDATE: Added support for 3 new coordinate formats (WKT, WKB, GeoJSON/JSON)
    - Added MGRS Go To and Plot Polygon functionality (Sentinel-2 compatible)
    - Fixed critical MGRS coordinate conversion bug (latitude band cycle calculation)
    - Made X and Y inputs editable for manual coordinate entry
    - Implemented smart geometry type detection for all formats
    - Added proper symbology for Point, LineString, Polygon, and Multi geometries
    - Color-coded visualization: Red (XYZ), Blue (MGRS), Green (WKT), Yellow (WKB), Purple (GeoJSON)
    - Enhanced GeoJSON parser supporting all geometry types including Multi
    - Improved error handling with detailed user feedback messages
    - Updated tooltips to reflect new multi-format capabilities
    - Added geometry type display in layer attributes
    - Fixed WKB hex string parsing and conversion
    - Optimized memory layer creation for different geometry types
    - Enhanced Go To function with automatic extent buffering (10 percent)
    - Updated dock widget to support 5 coordinate systems with dynamic input fields
    .
    Version 0.1 (2025-08-15)
    - Initial release
    - XYZ tile coordinate capture from map clicks
    - MGRS grid reference capture from map clicks
    - Dual coordinate system support with dropdown selection
    - Interactive crosshair cursor for precise coordinate capture
    - XYZ tile navigation (Go To functionality)
    - XYZ tile polygon plotting with red outline visualization
    - Zoom level control for XYZ tiles (0-22 range)
    - Professional dockable widget interface
    - Integration with MAS Raster Processing menu and toolbar
    - Smart toolbar behavior with proper tool state management
    - Dock widget persistence when switching tools
    - Status bar feedback and message notifications
    - Error handling with user-friendly messages
    - Memory layer creation with proper attribute tables
    - Coordinate reprojection support for different CRS
    - Professional tooltips and help documentation

server=False
